**Q: How do I change my setup after the Extender is up and running?**

**A:**

Make sure you are on a PC that is connected to the Extender network and your PC is configured as DHCP client mode.

In your browser, type the address: **192.168.20.1**.

If you still cannot access the Extender, close your browser. Then open a new browser and type **192.168.20.1**.