**Q: What is the maximum link rate in KA1750 11ac mode?**

**A:**
If you use 11n wireless devices to connect with KA1750, the maximum connection link rate is 1300Mbps. To take advantage of the higher 802.11ac Wi-Fi speeds you will require an 802.11ac client device.